# Static Call Graph for image .\relay_8.axf

#<CALLGRAPH># ARM Linker, 5050106: Last Updated: Tue Nov 07 21:44:26 2017

### Maximum Stack Usage = 384 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

Operate_READ_RELAY ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Get_Switch1 from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Get_Switch2 from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Get_Switch3 from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Get_Switch4 from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - HardFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Operate_ALARM from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_GET_INPUT from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_GET_NONC from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_HOST from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_READ_RELAY from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_SCAN_DEVICE from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_SET_ALARM from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_SET_ALL from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_SET_NONC from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_SET_PORT from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_SET_RELAY from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_SET_SW from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Operate_STATE from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Relay1_OFF from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay1_ON from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay2_OFF from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay2_ON from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay3_OFF from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay3_ON from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay4_OFF from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay4_ON from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay5_OFF from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay5_ON from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay6_OFF from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay6_ON from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay7_OFF from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay7_ON from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay8_OFF from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Relay8_ON from app_processevents.o(.text) referenced from app_processevents.o(.constdata)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x.o(.text) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from wifi.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from sim800c.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from wifi.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from wifi.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f10x_hd.o(.text)
  - _sputc from printf8.o(i._sputc) referenced from printf8.o(i.__0sprintf$8)
  - fputc from wifi.o(.text) referenced from printf8.o(i.__0printf$8)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  SystemReset (Thumb, 16 bytes, Stack size 0 bytes, httputil.o(.emb_text))
  [Called By]

  - >> key_process
  - >> check_init_state

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  SystemCoreClockUpdate (Thumb, 142 bytes, Stack size 8 bytes, system_stm32f10x.o(.text), UNUSED)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> HOCO_TIM1_init
  - >> TIM4_Int_Init
  - >> TIM3_Int_Init
  - >> HCHO_Usart1_Init
  - >> net_usart2
  - >> com_usart1
  - >> TIM2_Int_Init
  - >> timer1_init
  - >> com_usart3

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> delay_init

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> beep_init
  - >> Key_Init
  - >> HCHO_Usart1_Init
  - >> open_sim800_pwr
  - >> net_usart2
  - >> hcho_adc_Init
  - >> com_usart1
  - >> set_pm25_rst_pin
  - >> hcho_is_ok
  - >> fan_init
  - >> at24c16_init
  - >> WIZ_SPI_Init
  - >> GPIO_Configuration
  - >> IIC_Init
  - >> com_usart3
  - >> net_gpio
  - >> relay_init

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> key_process
  - >> hcho_is_ok
  - >> clock
  - >> read_1byte
  - >> Get_Switch4
  - >> Get_Switch3
  - >> Get_Switch2
  - >> Get_Switch1

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> set_alarm
  - >> timer2_irq
  - >> beep_di
  - >> open_sim800_pwr
  - >> set_pm25_rst_pin
  - >> fan_on
  - >> at24c16_start
  - >> write_1byte
  - >> clock
  - >> read_1byte
  - >> at24c16_stop
  - >> WIZ_SPI_Init
  - >> WIZ_CS
  - >> Reset_W5500
  - >> GPIO_Configuration
  - >> IIC_Init
  - >> net_gpio
  - >> Relay8_ON
  - >> Relay7_ON
  - >> Relay6_ON
  - >> Relay5_ON
  - >> Relay4_ON
  - >> Relay3_ON
  - >> Relay2_ON
  - >> Relay1_ON

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> set_alarm
  - >> timer2_irq
  - >> beep_di
  - >> beep_init
  - >> fan_off
  - >> at24c16_start
  - >> write_1byte
  - >> clock
  - >> read_1byte
  - >> at24c16_stop
  - >> WIZ_CS
  - >> Reset_W5500
  - >> Relay8_OFF
  - >> Relay7_OFF
  - >> Relay6_OFF
  - >> Relay5_OFF
  - >> Relay4_OFF
  - >> Relay3_OFF
  - >> Relay2_OFF
  - >> Relay1_OFF

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 138 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinRemapConfig
  [Called By]
  - >> HCHO_Usart1_Init
  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  GPIO_EXTILineConfig (Thumb, 66 bytes, Stack size 12 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> System_RCC_Configuration1

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_GetFlagStatus
  [Called By]
  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration
  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus
  [Called By]
  - >> System_RCC_Configuration1

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> System_RCC_Configuration

  RCC_PLLConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  RCC_SYSCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  RCC_HCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  RCC_PCLK1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  RCC_PCLK2Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  RCC_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  RCC_LSEConfig (Thumb, 50 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> I2S_Init
  - >> USART_Init

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> HOCO_TIM1_init
  - >> HCHO_Usart1_Init
  - >> System_RCC_Configuration1
  - >> hcho_adc_Init
  - >> System_RCC_Configuration
  - >> fan_init
  - >> at24c16_init
  - >> WIZ_SPI_Init
  - >> GPIO_Configuration
  - >> IIC_Init
  - >> timer1_init

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> TIM4_Int_Init
  - >> TIM3_Int_Init
  - >> System_RCC_Configuration1
  - >> net_usart2
  - >> TIM2_Int_Init
  - >> System_RCC_Configuration
  - >> com_usart3

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> SPI_I2S_DeInit
  - >> TIM_DeInit
  - >> ADC_DeInit
  - >> USART_DeInit
  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> SPI_I2S_DeInit
  - >> TIM_DeInit
  - >> USART_DeInit

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  USART_Init (Thumb, 210 bytes, Stack size 56 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> HCHO_Usart1_Init
  - >> net_usart2
  - >> com_usart1
  - >> com_usart3

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 34 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> HCHO_Usart1_Init
  - >> net_usart2
  - >> com_usart1
  - >> com_usart3

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> HCHO_Usart1_Init
  - >> net_usart2
  - >> com_usart1
  - >> com_usart3

  USART_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> sim800_send
  - >> com_send
  - >> USART2_Puts
  - >> USART2_Putc
  - >> fputc

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler
  - >> USART2_IRQHandler
  - >> USART3_IRQHandler

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> sim800_send
  - >> com_send
  - >> USART2_Puts
  - >> USART2_Putc
  - >> fputc

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetITStatus (Thumb, 84 bytes, Stack size 16 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler
  - >> USART2_IRQHandler
  - >> USART3_IRQHandler

  USART_ClearITPendingBit (Thumb, 52 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_ClearITPendingBit
  [Called By]
  - >> USART1_IRQHandler
  - >> USART2_IRQHandler
  - >> USART3_IRQHandler

  ADC_DeInit (Thumb, 78 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_DeInit
  [Calls]
  - >> RCC_APB2PeriphResetCmd
  [Called By]
  - >> hcho_adc_Init

  ADC_Init (Thumb, 70 bytes, Stack size 12 bytes, stm32f10x_adc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = ADC_Init
  [Called By]
  - >> hcho_adc_Init

  ADC_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> hcho_adc_Init

  ADC_DMACmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_ITConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_ResetCalibration (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> hcho_adc_Init

  ADC_GetResetCalibrationStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> hcho_adc_Init

  ADC_StartCalibration (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> hcho_adc_Init

  ADC_GetCalibrationStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> hcho_adc_Init

  ADC_SoftwareStartConvCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> hm_adc_sample
  - >> hcho_adc_sample

  ADC_GetSoftwareStartConvStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_DiscModeChannelCountConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_DiscModeCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_RegularChannelConfig (Thumb, 184 bytes, Stack size 20 bytes, stm32f10x_adc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = ADC_RegularChannelConfig
  [Called By]
  - >> hm_adc_sample
  - >> hcho_adc_sample

  ADC_ExternalTrigConvCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_GetConversionValue (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> hm_adc_sample
  - >> hcho_adc_sample

  ADC_GetDualModeConversionValue (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_AutoInjectedConvCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_InjectedDiscModeCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_ExternalTrigInjectedConvConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_ExternalTrigInjectedConvCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_SoftwareStartInjectedConvCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_GetSoftwareStartInjectedConvCmdStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_InjectedChannelConfig (Thumb, 130 bytes, Stack size 20 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_InjectedSequencerLengthConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_SetInjectedOffset (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_GetInjectedConversionValue (Thumb, 28 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_AnalogWatchdogCmd (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_AnalogWatchdogThresholdsConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_AnalogWatchdogSingleChannelConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_TempSensorVrefintCmd (Thumb, 64 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> hcho_adc_Init

  ADC_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> hm_adc_sample
  - >> hcho_adc_sample

  ADC_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> hm_adc_sample
  - >> hcho_adc_sample

  ADC_GetITStatus (Thumb, 36 bytes, Stack size 16 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_ClearITPendingBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  TIM_DeInit (Thumb, 424 bytes, Stack size 8 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  TIM_TimeBaseInit (Thumb, 122 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> HOCO_TIM1_init
  - >> TIM4_Int_Init
  - >> TIM3_Int_Init
  - >> TIM2_Int_Init
  - >> timer1_init

  TIM_OC1Init (Thumb, 132 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2Init (Thumb, 154 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3Init (Thumb, 150 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4Init (Thumb, 182 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetIC4Prescaler (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC3Prescaler (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC2Prescaler (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_SetIC1Prescaler (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_ICInit (Thumb, 150 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TIM_SetIC3Prescaler
  - >> TIM_SetIC4Prescaler
  - >> TI1_Config
  - >> TI2_Config
  - >> TI3_Config
  - >> TI4_Config

  TIM_PWMIConfig (Thumb, 124 bytes, Stack size 24 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TI1_Config
  - >> TI2_Config

  TIM_BDTRConfig (Thumb, 32 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_TimeBaseStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OCStructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ICStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_BDTRStructInit (Thumb, 40 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> HOCO_TIM1_init
  - >> TIM4_Int_Init
  - >> TIM3_Int_Init
  - >> TIM2_Int_Init
  - >> timer1_init
  - >> start_smartlink_timer2
  - >> close_smartlink_timer2
  - >> close_net_interval
  - >> start_com_interval
  - >> start_net_interval

  TIM_CtrlPWMOutputs (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> HOCO_TIM1_init
  - >> TIM4_Int_Init
  - >> TIM3_Int_Init
  - >> TIM2_Int_Init
  - >> timer1_init

  TIM_GenerateEvent (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_DMAConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_InternalClockConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectInputTrigger (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_ITRxExternalClockConfig

  TIM_ITRxExternalClockConfig (Thumb, 24 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger

  TIM_TIxExternalClockConfig (Thumb, 62 bytes, Stack size 24 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger
  - >> TI1_Config
  - >> TI2_Config

  TIM_ETRConfig (Thumb, 28 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ETRClockMode2Config
  - >> TIM_ETRClockMode1Config

  TIM_ETRClockMode1Config (Thumb, 54 bytes, Stack size 24 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_ETRClockMode2Config (Thumb, 32 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_PrescalerConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CounterModeConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_EncoderInterfaceConfig (Thumb, 66 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC2Config (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC3Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC4Config (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ARRPreloadConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectCOM (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectCCDMA (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCPreloadControl (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1FastConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2FastConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3FastConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4FastConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC1Ref (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC2Ref (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC3Ref (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC4Ref (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1PolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1NPolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCxCmd (Thumb, 30 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCxNCmd (Thumb, 30 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOCxM (Thumb, 82 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_UpdateDisableConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_UpdateRequestConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectHallSensor (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOnePulseMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOutputTrigger (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectMasterSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetAutoreload (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare1 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare2 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare3 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare4 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetClockDivision (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture1 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture2 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture3 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture4 (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCounter (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetPrescaler (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetITStatus (Thumb, 34 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_GetITStatus
  [Called By]
  - >> timer2_irq
  - >> TIM1_UP_IRQHandler

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> timer2_irq
  - >> TIM1_UP_IRQHandler

  FLASH_SetLatency (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  FLASH_HalfCycleAccessCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_PrefetchBufferCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text))
  [Called By]

  - >> System_RCC_Configuration1
  - >> System_RCC_Configuration

  FLASH_Unlock (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_UnlockBank1 (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_Lock (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_LockBank1 (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetBank1Status (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Called By]

  - >> FLASH_WaitForLastBank1Operation
  - >> FLASH_WaitForLastOperation

  FLASH_WaitForLastOperation (Thumb, 38 bytes, Stack size 4 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_GetBank1Status
  [Called By]
  - >> FLASH_UserOptionByteConfig
  - >> FLASH_ReadOutProtection
  - >> FLASH_EnableWriteProtection
  - >> FLASH_ProgramOptionByteData
  - >> FLASH_ProgramHalfWord
  - >> FLASH_ProgramWord
  - >> FLASH_EraseOptionBytes
  - >> FLASH_EraseAllPages
  - >> FLASH_ErasePage

  FLASH_ErasePage (Thumb, 72 bytes, Stack size 12 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_EraseAllPages (Thumb, 68 bytes, Stack size 8 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_WaitForLastBank1Operation (Thumb, 38 bytes, Stack size 4 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_GetBank1Status
  [Called By]
  - >> FLASH_EraseAllBank1Pages

  FLASH_EraseAllBank1Pages (Thumb, 68 bytes, Stack size 8 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastBank1Operation

  FLASH_GetReadOutProtectionStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Called By]

  - >> FLASH_EraseOptionBytes

  FLASH_EraseOptionBytes (Thumb, 150 bytes, Stack size 12 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_GetReadOutProtectionStatus
  - >> FLASH_WaitForLastOperation

  FLASH_ProgramWord (Thumb, 102 bytes, Stack size 20 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_ProgramHalfWord (Thumb, 60 bytes, Stack size 16 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_ProgramOptionByteData (Thumb, 72 bytes, Stack size 16 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_EnableWriteProtection (Thumb, 200 bytes, Stack size 28 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_ReadOutProtection (Thumb, 156 bytes, Stack size 12 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_UserOptionByteConfig (Thumb, 88 bytes, Stack size 20 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_GetUserOptionByte (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetWriteProtectionOptionByte (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetPrefetchBufferStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetFlagStatus (Thumb, 42 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetStatus (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  SPI_I2S_DeInit (Thumb, 76 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  SPI_Init (Thumb, 60 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Called By]

  - >> WIZ_SPI_Init

  I2S_Init (Thumb, 226 bytes, Stack size 56 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetClocksFreq

  SPI_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  I2S_StructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Called By]

  - >> WIZ_SPI_Init

  I2S_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ITConfig (Thumb, 32 bytes, Stack size 12 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Called By]

  - >> SPI2_SendByte

  SPI_I2S_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Called By]

  - >> SPI2_SendByte

  SPI_NSSInternalSoftwareConfig (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_DataSizeConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_CalculateCRC (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Called By]

  - >> SPI2_SendByte

  SPI_I2S_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetITStatus (Thumb, 52 bytes, Stack size 20 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)

  Delay_ms (Thumb, 44 bytes, Stack size 12 bytes, main.o(.text), UNUSED)
  [Called By]

  - >> at24c16_write
  - >> set_network
  - >> Reset_W5500

  set_pm25_rst_pin (Thumb, 38 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = set_pm25_rst_pin ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> main

  main (Thumb, 110 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 280
  - Call Chain = main ⇒ server_host_id ⇒ Encode ⇒ DES3 ⇒ DES ⇒ SubKey ⇒ RShift
  [Calls]
  - >> wifi_server_process
  - >> timer_signal_set
  - >> timer_all_init
  - >> sim800_run
  - >> server_host_id
  - >> server_client_clr
  - >> process_com_buf
  - >> open_sim800_pwr
  - >> net_val_init
  - >> net_usart2
  - >> hcho_adc_Init
  - >> delay_init
  - >> com_usart1
  - >> com_init
  - >> TIM2_Int_Init
  - >> System_RCC_Configuration
  - >> NVIC_Configuration
  - >> set_pm25_rst_pin
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  System_RCC_Configuration1 (Thumb, 212 bytes, Stack size 8 bytes, stm32config.o(.text), UNUSED)
  [Calls]

  - >> FLASH_PrefetchBufferCmd
  - >> FLASH_SetLatency
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHBPeriphClockCmd
  - >> RCC_ADCCLKConfig
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HCLKConfig
  - >> RCC_GetSYSCLKSource
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLCmd
  - >> RCC_PLLConfig
  - >> RCC_WaitForHSEStartUp
  - >> RCC_GetFlagStatus
  - >> RCC_HSEConfig
  - >> RCC_DeInit
  - >> GPIO_PinRemapConfig

  System_RCC_Configuration (Thumb, 214 bytes, Stack size 8 bytes, stm32config.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = System_RCC_Configuration ⇒ GPIO_PinRemapConfig
  [Calls]
  - >> FLASH_PrefetchBufferCmd
  - >> FLASH_SetLatency
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHBPeriphClockCmd
  - >> RCC_ADCCLKConfig
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HCLKConfig
  - >> RCC_GetSYSCLKSource
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLCmd
  - >> RCC_PLLConfig
  - >> RCC_HSICmd
  - >> RCC_GetFlagStatus
  - >> RCC_DeInit
  - >> GPIO_PinRemapConfig
  [Called By]
  - >> main

  NVIC_Configuration (Thumb, 22 bytes, Stack size 8 bytes, stm32config.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = NVIC_Configuration
  [Calls]
  - >> NVIC_SetVectorTable
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> main

  HCHO_Usart1_Init (Thumb, 162 bytes, Stack size 32 bytes, stm32config.o(.text), UNUSED)
  [Calls]

  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_PinRemapConfig
  - >> GPIO_Init
  - >> NVIC_Init

  TIM3_Int_Init (Thumb, 90 bytes, Stack size 32 bytes, stm32config.o(.text), UNUSED)
  [Calls]

  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init

  TIM4_Int_Init (Thumb, 90 bytes, Stack size 32 bytes, stm32config.o(.text), UNUSED)
  [Calls]

  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init

  HOCO_TIM1_init (Thumb, 94 bytes, Stack size 32 bytes, stm32config.o(.text), UNUSED)
  [Calls]

  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  - >> RCC_APB2PeriphClockCmd
  - >> NVIC_Init

  Key_Init (Thumb, 30 bytes, Stack size 8 bytes, stm32config.o(.text), UNUSED)
  [Calls]

  - >> GPIO_Init

  beep_init (Thumb, 38 bytes, Stack size 8 bytes, stm32config.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ResetBits
  - >> GPIO_Init

  beep_di (Thumb, 44 bytes, Stack size 8 bytes, stm32config.o(.text), UNUSED)
  [Calls]

  - >> delay_ms
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> beep_didididi
  - >> beep_didi

  beep_didi (Thumb, 12 bytes, Stack size 8 bytes, stm32config.o(.text), UNUSED)
  [Calls]

  - >> beep_di

  beep_didididi (Thumb, 20 bytes, Stack size 8 bytes, stm32config.o(.text), UNUSED)
  [Calls]

  - >> beep_di

  key_process (Thumb, 68 bytes, Stack size 8 bytes, stm32config.o(.text), UNUSED)
  [Calls]

  - >> write_ip_pri
  - >> write_eeprom_flag
  - >> set_default_reset
  - >> SystemReset
  - >> GPIO_ReadInputDataBit
  - >> __2printf

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32f10x_it.o(.text))
  [Stack]

  - Max Depth = 240
  - Call Chain = TIM2_IRQHandler ⇒ timer2_irq ⇒ sync_data ⇒ send_sync_data ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> timer2_irq
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  relay_init (Thumb, 88 bytes, Stack size 8 bytes, app_processevents.o(.text), UNUSED)
  [Calls]

  - >> GPIO_Init

  cmd_para_init (Thumb, 24 bytes, Stack size 8 bytes, app_processevents.o(.text), UNUSED)
  [Calls]

  - >> AT24C02_Read

  Relay1_ON (Thumb, 12 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay1_ON
  [Calls]
  - >> GPIO_SetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay2_ON (Thumb, 12 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay2_ON
  [Calls]
  - >> GPIO_SetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay3_ON (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay3_ON
  [Calls]
  - >> GPIO_SetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay4_ON (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay4_ON
  [Calls]
  - >> GPIO_SetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay5_ON (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay5_ON
  [Calls]
  - >> GPIO_SetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay6_ON (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay6_ON
  [Calls]
  - >> GPIO_SetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay7_ON (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay7_ON
  [Calls]
  - >> GPIO_SetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay8_ON (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay8_ON
  [Calls]
  - >> GPIO_SetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay1_OFF (Thumb, 12 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay1_OFF
  [Calls]
  - >> GPIO_ResetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay2_OFF (Thumb, 12 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay2_OFF
  [Calls]
  - >> GPIO_ResetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay3_OFF (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay3_OFF
  [Calls]
  - >> GPIO_ResetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay4_OFF (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay4_OFF
  [Calls]
  - >> GPIO_ResetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay5_OFF (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay5_OFF
  [Calls]
  - >> GPIO_ResetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay6_OFF (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay6_OFF
  [Calls]
  - >> GPIO_ResetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay7_OFF (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay7_OFF
  [Calls]
  - >> GPIO_ResetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Relay8_OFF (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Relay8_OFF
  [Calls]
  - >> GPIO_ResetBits
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Get_Switch1 (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Get_Switch1
  [Calls]
  - >> GPIO_ReadInputDataBit
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Get_Switch2 (Thumb, 14 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Get_Switch2
  [Calls]
  - >> GPIO_ReadInputDataBit
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Get_Switch3 (Thumb, 12 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Get_Switch3
  [Calls]
  - >> GPIO_ReadInputDataBit
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Get_Switch4 (Thumb, 12 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Get_Switch4
  [Calls]
  - >> GPIO_ReadInputDataBit
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  set_relay (Thumb, 54 bytes, Stack size 16 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = set_relay
  [Called By]
  - >> Operate_SET_RELAY
  - >> set_8_relay

  set_8_relay (Thumb, 42 bytes, Stack size 16 bytes, app_processevents.o(.text), UNUSED)
  [Calls]

  - >> set_relay

  get_8_relay (Thumb, 28 bytes, Stack size 0 bytes, app_processevents.o(.text), UNUSED)

  get_relay (Thumb, 20 bytes, Stack size 0 bytes, app_processevents.o(.text), UNUSED)

  Alarm_Signl_Set (Thumb, 44 bytes, Stack size 8 bytes, app_processevents.o(.text), UNUSED)
  [Calls]

  - >> timer_signal_set
  - >> timer_get_run
  [Called By]
  - >> alarm_process

  alarm_process (Thumb, 90 bytes, Stack size 8 bytes, app_processevents.o(.text), UNUSED)
  [Calls]

  - >> Send_Alarm_Message
  - >> Switch_State_Scan
  - >> Alarm_Signl_Set

  Stop_Alarm_Resend (Thumb, 14 bytes, Stack size 0 bytes, app_processevents.o(.text))
  [Called By]

  - >> Operate_ALARM

  Para_Write (Thumb, 50 bytes, Stack size 32 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = Para_Write ⇒ AT24C02_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> AT24C02_WriteOneByte
  [Called By]
  - >> Operate_SET_PORT
  - >> Operate_SET_ALARM
  - >> Operate_SET_SW
  - >> Operate_SET_NONC
  - >> Operate_SET_RELAY

  SET_RELAY (Thumb, 20 bytes, Stack size 8 bytes, app_processevents.o(.text), UNUSED)
  [Calls]

  - >> Get_Set
  - >> set_alarm

  Alarm_Resend (Thumb, 100 bytes, Stack size 8 bytes, app_processevents.o(.text), UNUSED)
  [Calls]

  - >> Send_Alarm_Message
  - >> timer_signal_set
  - >> timer_get_state
  - >> timer_clr_state

  Operate_SET_RELAY (Thumb, 414 bytes, Stack size 88 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 376
  - Call Chain = Operate_SET_RELAY ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> SplitData
  - >> Parameter_Check
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> Net_SendReply
  - >> Para_Write
  - >> set_relay
  - >> __2sprintf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_READ_RELAY (Thumb, 278 bytes, Stack size 96 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 384
  - Call Chain = Operate_READ_RELAY ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> Parameter_Check
  - >> strchr
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> Net_SendReply
  - >> atoi
  - >> __2sprintf
  - >> __2printf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_STATE (Thumb, 190 bytes, Stack size 80 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 368
  - Call Chain = Operate_STATE ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> Get_Set
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> Net_SendReply
  - >> atoi
  - >> __2sprintf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_GET_INPUT (Thumb, 196 bytes, Stack size 80 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 368
  - Call Chain = Operate_GET_INPUT ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> read_input
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> Net_SendReply
  - >> atoi
  - >> __2sprintf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_ALARM (Thumb, 92 bytes, Stack size 24 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = Operate_ALARM ⇒ atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> Parameter_Check
  - >> strcmp
  - >> strchr
  - >> Stop_Alarm_Resend
  - >> atoi
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_SET_NONC (Thumb, 366 bytes, Stack size 88 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 376
  - Call Chain = Operate_SET_NONC ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> SplitData
  - >> Parameter_Check
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> Net_SendReply
  - >> Para_Write
  - >> __2sprintf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_GET_NONC (Thumb, 196 bytes, Stack size 80 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 368
  - Call Chain = Operate_GET_NONC ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> Get_Set
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> Net_SendReply
  - >> atoi
  - >> __2sprintf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_SET_SW (Thumb, 310 bytes, Stack size 88 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 376
  - Call Chain = Operate_SET_SW ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> SplitData
  - >> Parameter_Check
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> Net_SendReply
  - >> Para_Write
  - >> __2sprintf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_SET_ALARM (Thumb, 306 bytes, Stack size 88 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 376
  - Call Chain = Operate_SET_ALARM ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> SplitData
  - >> Parameter_Check
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> Net_SendReply
  - >> Para_Write
  - >> __2sprintf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_SET_PORT (Thumb, 288 bytes, Stack size 88 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 376
  - Call Chain = Operate_SET_PORT ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> strchr
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> Net_SendReply
  - >> Para_Write
  - >> atoi
  - >> __2sprintf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_SET_ALL (Thumb, 280 bytes, Stack size 96 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 384
  - Call Chain = Operate_SET_ALL ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> strchr
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> Net_SendReply
  - >> atoi
  - >> __2sprintf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_SCAN_DEVICE (Thumb, 42 bytes, Stack size 64 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 352
  - Call Chain = Operate_SCAN_DEVICE ⇒ Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> __aeabi_memclr4
  - >> Net_SendReply
  - >> __2sprintf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  Operate_HOST (Thumb, 70 bytes, Stack size 96 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 232
  - Call Chain = Operate_HOST ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> Test_Relay
  - >> strlen
  - >> __aeabi_memclr4
  - >> server_get_id
  - >> Send_Mode
  - >> __2sprintf
  [Address Reference Count : 1]
  - app_processevents.o(.constdata)

  app_process_cmd (Thumb, 154 bytes, Stack size 232 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 256
  - Call Chain = app_process_cmd ⇒ __2printf
  [Calls]
  - >> strcmp
  - >> strchr
  - >> __aeabi_memclr4
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> wifi_server_process
  - >> com_process

  delay_init (Thumb, 42 bytes, Stack size 8 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_init
  [Calls]
  - >> SysTick_CLKSourceConfig
  [Called By]
  - >> main

  delay_us (Thumb, 72 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> IIC_Read_Byte
  - >> IIC_Send_Byte
  - >> IIC_NAck
  - >> IIC_Ack
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start

  delay_ms (Thumb, 72 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> Test_Relay
  - >> beep_di
  - >> net_send
  - >> net_hardware_err
  - >> AT24C02_WriteOneByte

  net_hardware_err (Thumb, 28 bytes, Stack size 0 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> delay_ms

  net_gpio (Thumb, 38 bytes, Stack size 8 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> GPIO_SetBits
  - >> GPIO_Init

  net_clr_com_state (Thumb, 12 bytes, Stack size 0 bytes, wifi.o(.text))
  [Called By]

  - >> server_login
  - >> server_handle
  - >> net_cmd_handle

  net_com_state (Thumb, 6 bytes, Stack size 0 bytes, wifi.o(.text))
  [Called By]

  - >> net_cmd_handle

  com_clr_com_state (Thumb, 12 bytes, Stack size 0 bytes, wifi.o(.text), UNUSED)
  [Called By]

  - >> com_cmd_handle

  com_com_state (Thumb, 6 bytes, Stack size 0 bytes, wifi.o(.text), UNUSED)
  [Called By]

  - >> com_cmd_handle

  net_usart2 (Thumb, 154 bytes, Stack size 32 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = net_usart2 ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_Init
  - >> RCC_APB1PeriphClockCmd
  - >> GPIO_Init
  - >> NVIC_Init
  [Called By]
  - >> main

  com_usart3 (Thumb, 160 bytes, Stack size 32 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = com_usart3 ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_Init
  - >> RCC_APB1PeriphClockCmd
  - >> GPIO_Init
  - >> NVIC_Init
  [Called By]
  - >> com_init

  fputc (Thumb, 32 bytes, Stack size 16 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_GetFlagStatus
  - >> USART_SendData
  [Address Reference Count : 1]
  - printf8.o(i.__0printf$8)

  USART2_Putc (Thumb, 28 bytes, Stack size 8 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> USART_GetFlagStatus
  - >> USART_SendData

  USART2_Puts (Thumb, 38 bytes, Stack size 8 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> USART_GetFlagStatus
  - >> USART_SendData

  GetKey (Thumb, 26 bytes, Stack size 0 bytes, wifi.o(.text), UNUSED)

  start_net_interval (Thumb, 56 bytes, Stack size 8 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> TIM_Cmd

  start_com_interval (Thumb, 54 bytes, Stack size 8 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> TIM_Cmd

  close_net_interval (Thumb, 12 bytes, Stack size 8 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = close_net_interval
  [Calls]
  - >> TIM_Cmd
  [Called By]
  - >> TIM1_UP_IRQHandler

  TIM1_UP_IRQHandler (Thumb, 136 bytes, Stack size 8 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM1_UP_IRQHandler ⇒ TIM_GetITStatus
  [Calls]
  - >> TIM_ClearITPendingBit
  - >> TIM_GetITStatus
  - >> close_net_interval
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  net_clr_rx_buf (Thumb, 12 bytes, Stack size 0 bytes, wifi.o(.text))
  [Called By]

  - >> net_val_init

  com_clr_rx_buf (Thumb, 12 bytes, Stack size 0 bytes, wifi.o(.text), UNUSED)
  [Called By]

  - >> com_val_init

  net_buffer_input (Thumb, 108 bytes, Stack size 0 bytes, wifi.o(.text))
  [Called By]

  - >> sim800_run
  - >> sim800_recevie

  net_buffer_output (Thumb, 78 bytes, Stack size 0 bytes, wifi.o(.text))
  [Called By]

  - >> Check_Net_Stat
  - >> server_handle
  - >> net_cmd_handle
  - >> buffer_output
  - >> net_buffer_output_num

  com_buffer_output (Thumb, 78 bytes, Stack size 0 bytes, wifi.o(.text), UNUSED)
  [Called By]

  - >> com_cmd_handle
  - >> buffer_output
  - >> com_buffer_output_num

  net_buffer_output_num (Thumb, 36 bytes, Stack size 12 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> net_buffer_output

  com_buffer_output_num (Thumb, 36 bytes, Stack size 12 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> com_buffer_output

  net_val_init (Thumb, 26 bytes, Stack size 8 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = net_val_init ⇒ server_client_clr
  [Calls]
  - >> server_client_clr
  - >> __aeabi_memclr4
  - >> net_clr_rx_buf
  [Called By]
  - >> main

  com_val_init (Thumb, 22 bytes, Stack size 8 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memclr4
  - >> com_clr_rx_buf

  set_net_interval (Thumb, 10 bytes, Stack size 0 bytes, wifi.o(.text), UNUSED)

  clr_buf (Thumb, 22 bytes, Stack size 8 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = clr_buf
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> read_pm

  add_one_byte (Thumb, 32 bytes, Stack size 0 bytes, wifi.o(.text))
  [Called By]

  - >> USART2_IRQHandler

  del_one_byte (Thumb, 24 bytes, Stack size 0 bytes, wifi.o(.text), UNUSED)

  get_buf_len (Thumb, 44 bytes, Stack size 0 bytes, wifi.o(.text))
  [Called By]

  - >> process_com_buf
  - >> del_bytes

  del_bytes (Thumb, 50 bytes, Stack size 4 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> get_buf_len

  atohex (Thumb, 38 bytes, Stack size 0 bytes, wifi.o(.text), UNUSED)
  [Called By]

  - >> chartohex

  chartohex (Thumb, 34 bytes, Stack size 12 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> atohex

  process_com_buf (Thumb, 48 bytes, Stack size 4 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = process_com_buf
  [Calls]
  - >> get_buf_len
  [Called By]
  - >> main

  USART3_IRQHandler (Thumb, 34 bytes, Stack size 8 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART3_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ClearITPendingBit
  - >> USART_GetITStatus
  - >> USART_ReceiveData
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 40 bytes, Stack size 8 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART2_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ClearITPendingBit
  - >> USART_GetITStatus
  - >> USART_ReceiveData
  - >> add_one_byte
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  com_init (Thumb, 12 bytes, Stack size 8 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = com_init ⇒ com_usart3 ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> com_usart3
  [Called By]
  - >> main

  net_send (Thumb, 64 bytes, Stack size 40 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = net_send ⇒ sim800_send
  [Calls]
  - >> delay_ms
  - >> sim800_send
  [Called By]
  - >> ZLN_Read
  - >> server_send

  com_send (Thumb, 44 bytes, Stack size 16 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = com_send
  [Calls]
  - >> USART_GetFlagStatus
  - >> USART_SendData
  [Called By]
  - >> read_pm

  AscToNum (Thumb, 30 bytes, Stack size 0 bytes, wifi.o(.text), UNUSED)

  buffer_output (Thumb, 26 bytes, Stack size 8 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> com_buffer_output
  - >> net_buffer_output

  cmd_analysis (Thumb, 6 bytes, Stack size 0 bytes, wifi.o(.text), UNUSED)

  net_cmd_handle (Thumb, 132 bytes, Stack size 16 bytes, wifi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = net_cmd_handle
  [Calls]
  - >> __aeabi_memclr4
  - >> net_buffer_output
  - >> net_com_state
  - >> net_clr_com_state
  [Called By]
  - >> wifi_server_process

  com_cmd_handle (Thumb, 164 bytes, Stack size 16 bytes, wifi.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memclr4
  - >> com_buffer_output
  - >> com_com_state
  - >> com_clr_com_state
  [Called By]
  - >> com_process

  DES (Thumb, 180 bytes, Stack size 24 bytes, des.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = DES ⇒ SubKey ⇒ RShift
  [Calls]
  - >> __aeabi_memcpy
  - >> P
  - >> S
  - >> EXP
  - >> SubKey
  - >> InitKey
  - >> EP
  - >> IP
  - >> Xor
  - >> ShrinkBit
  - >> ExpandBit
  [Called By]
  - >> Decode
  - >> Encode
  - >> DES3

  DES3 (Thumb, 102 bytes, Stack size 24 bytes, des.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = DES3 ⇒ DES ⇒ SubKey ⇒ RShift
  [Calls]
  - >> DES
  [Called By]
  - >> Decode
  - >> Encode

  Encode (Thumb, 136 bytes, Stack size 40 bytes, des.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = Encode ⇒ DES3 ⇒ DES ⇒ SubKey ⇒ RShift
  [Calls]
  - >> DES3
  - >> DES
  [Called By]
  - >> server_host_id

  Decode (Thumb, 60 bytes, Stack size 32 bytes, des.o(.text), UNUSED)
  [Calls]

  - >> DES3
  - >> DES

  server_read_mcu_id (Thumb, 38 bytes, Stack size 24 bytes, server.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = server_read_mcu_id ⇒ __2sprintf
  [Calls]
  - >> __2sprintf
  [Called By]
  - >> server_host_id

  server_host_id (Thumb, 226 bytes, Stack size 152 bytes, server.o(.text))
  [Stack]

  - Max Depth = 280
  - Call Chain = server_host_id ⇒ Encode ⇒ DES3 ⇒ DES ⇒ SubKey ⇒ RShift
  [Calls]
  - >> __aeabi_memclr4
  - >> server_read_mcu_id
  - >> Encode
  [Called By]
  - >> main

  server_check_lic (Thumb, 26 bytes, Stack size 8 bytes, server.o(.text), UNUSED)
  [Calls]

  - >> memcmp

  server_get_id (Thumb, 16 bytes, Stack size 8 bytes, server.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = server_get_id
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> server_handle
  - >> server_send
  - >> Operate_HOST

  server_send (Thumb, 146 bytes, Stack size 64 bytes, server.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy
  - >> net_send
  - >> server_get_id
  [Called By]
  - >> send_sync_data
  - >> server_heartbeat
  - >> server_login
  - >> Send_Mode

  server_add_client (Thumb, 176 bytes, Stack size 24 bytes, server.o(.text), UNUSED)
  [Calls]

  - >> memcmp

  server_client_clr (Thumb, 12 bytes, Stack size 8 bytes, server.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = server_client_clr
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> net_val_init
  - >> main
  - >> server_handle

  server_handle (Thumb, 528 bytes, Stack size 88 bytes, server.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = server_handle ⇒ __2printf
  [Calls]
  - >> timer_signal_set
  - >> server_client_clr
  - >> memcmp
  - >> timer_signal_init
  - >> net_buffer_output
  - >> net_clr_com_state
  - >> server_get_id
  - >> __2printf
  [Called By]
  - >> wifi_server_process

  server_login (Thumb, 42 bytes, Stack size 8 bytes, server.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = server_login ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> timer_signal_set
  - >> server_send
  - >> net_clr_com_state
  - >> __2printf
  [Called By]
  - >> wifi_server_process

  read_pm (Thumb, 24 bytes, Stack size 16 bytes, server.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = read_pm ⇒ com_send
  [Calls]
  - >> com_send
  - >> clr_buf
  [Called By]
  - >> server_heartbeat

  server_heartbeat (Thumb, 52 bytes, Stack size 8 bytes, server.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = server_heartbeat ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> timer_signal_set
  - >> read_pm
  - >> server_send
  - >> __2printf
  [Called By]
  - >> wifi_server_process

  server_err_process (Thumb, 50 bytes, Stack size 8 bytes, server.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = server_err_process ⇒ timer_signal_set
  [Calls]
  - >> timer_signal_set
  - >> timer_signal_init
  [Called By]
  - >> wifi_server_process

  wifi_server_process (Thumb, 108 bytes, Stack size 8 bytes, server.o(.text))
  [Stack]

  - Max Depth = 264
  - Call Chain = wifi_server_process ⇒ app_process_cmd ⇒ __2printf
  [Calls]
  - >> server_err_process
  - >> server_heartbeat
  - >> server_login
  - >> server_handle
  - >> net_cmd_handle
  - >> timer_get_state
  - >> app_process_cmd
  [Called By]
  - >> main

  com_process (Thumb, 22 bytes, Stack size 8 bytes, server.o(.text), UNUSED)
  [Calls]

  - >> com_cmd_handle
  - >> app_process_cmd

  ZLN_Read (Thumb, 46 bytes, Stack size 16 bytes, server.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy
  - >> net_send
  [Called By]
  - >> Check_Net_Stat

  Check_Net_Stat (Thumb, 70 bytes, Stack size 16 bytes, server.o(.text), UNUSED)
  [Calls]

  - >> ZLN_Read
  - >> net_buffer_output

  send_sync_data (Thumb, 20 bytes, Stack size 16 bytes, server.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = send_sync_data ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> server_send
  [Called By]
  - >> sync_data

  sync_data (Thumb, 68 bytes, Stack size 88 bytes, server.o(.text))
  [Stack]

  - Max Depth = 224
  - Call Chain = sync_data ⇒ send_sync_data ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> strlen
  - >> __aeabi_memclr4
  - >> send_sync_data
  - >> __2sprintf
  - >> __2printf
  [Called By]
  - >> timer2_irq

  Send_Mode (Thumb, 20 bytes, Stack size 16 bytes, server.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> server_send
  [Called By]
  - >> Net_SendReply
  - >> Operate_HOST

  Net_SendReply (Thumb, 116 bytes, Stack size 152 bytes, server.o(.text))
  [Stack]

  - Max Depth = 288
  - Call Chain = Net_SendReply ⇒ Send_Mode ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> strlen
  - >> strcat
  - >> __aeabi_memclr4
  - >> Send_Mode
  - >> __2printf
  [Called By]
  - >> Send_Alarm_Message
  - >> Operate_SCAN_DEVICE
  - >> Operate_SET_ALL
  - >> Operate_SET_PORT
  - >> Operate_SET_ALARM
  - >> Operate_SET_SW
  - >> Operate_GET_NONC
  - >> Operate_SET_NONC
  - >> Operate_GET_INPUT
  - >> Operate_STATE
  - >> Operate_READ_RELAY
  - >> Operate_SET_RELAY

  TIM2_Int_Init (Thumb, 92 bytes, Stack size 32 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = TIM2_Int_Init ⇒ NVIC_Init
  [Calls]
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  [Called By]
  - >> main

  close_smartlink_timer2 (Thumb, 20 bytes, Stack size 8 bytes, timer.o(.text), UNUSED)
  [Calls]

  - >> TIM_Cmd

  start_smartlink_timer2 (Thumb, 40 bytes, Stack size 8 bytes, timer.o(.text), UNUSED)
  [Calls]

  - >> TIM_Cmd

  timer2_irq (Thumb, 320 bytes, Stack size 8 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 232
  - Call Chain = timer2_irq ⇒ sync_data ⇒ send_sync_data ⇒ server_send ⇒ net_send ⇒ sim800_send
  [Calls]
  - >> TIM_ClearITPendingBit
  - >> TIM_GetITStatus
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> hm_adc_sample
  - >> hcho_adc_sample
  - >> Delay_us
  - >> sync_data
  [Called By]
  - >> TIM2_IRQHandler

  timer_all_init (Thumb, 12 bytes, Stack size 8 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = timer_all_init
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  timer_signal_init (Thumb, 20 bytes, Stack size 0 bytes, timer.o(.text))
  [Called By]

  - >> server_err_process
  - >> server_handle

  timer_signal_set (Thumb, 52 bytes, Stack size 8 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = timer_signal_set
  [Called By]
  - >> Switch_State_Scan
  - >> main
  - >> server_err_process
  - >> server_heartbeat
  - >> server_login
  - >> server_handle
  - >> Alarm_Resend
  - >> Alarm_Signl_Set

  timer_get_state (Thumb, 16 bytes, Stack size 0 bytes, timer.o(.text))
  [Called By]

  - >> Switch_State_Scan
  - >> wifi_server_process
  - >> Alarm_Resend

  timer_get_run (Thumb, 16 bytes, Stack size 0 bytes, timer.o(.text), UNUSED)
  [Called By]

  - >> Alarm_Signl_Set

  timer_clr_state (Thumb, 16 bytes, Stack size 0 bytes, timer.o(.text), UNUSED)
  [Called By]

  - >> Alarm_Resend

  timer1_init (Thumb, 98 bytes, Stack size 24 bytes, timer.o(.text), UNUSED)
  [Calls]

  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  - >> RCC_APB2PeriphClockCmd
  - >> NVIC_Init

  IIC_Init (Thumb, 50 bytes, Stack size 8 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> AT24C02_Init

  IIC_Start (Thumb, 64 bytes, Stack size 8 bytes, 24c02.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Start
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24C02_ReadOneByte
  - >> AT24C02_WriteOneByte

  IIC_Stop (Thumb, 66 bytes, Stack size 8 bytes, 24c02.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Stop
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24C02_ReadOneByte
  - >> IIC_Wait_Ack
  - >> AT24C02_WriteOneByte

  IIC_Wait_Ack (Thumb, 86 bytes, Stack size 8 bytes, 24c02.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_Wait_Ack ⇒ IIC_Stop
  [Calls]
  - >> IIC_Stop
  - >> delay_us
  [Called By]
  - >> AT24C02_ReadOneByte
  - >> AT24C02_WriteOneByte

  IIC_Ack (Thumb, 70 bytes, Stack size 8 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> delay_us
  [Called By]
  - >> IIC_Read_Byte

  IIC_NAck (Thumb, 70 bytes, Stack size 8 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> delay_us
  [Called By]
  - >> IIC_Read_Byte

  IIC_Send_Byte (Thumb, 104 bytes, Stack size 16 bytes, 24c02.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_Send_Byte
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24C02_ReadOneByte
  - >> AT24C02_WriteOneByte

  IIC_Read_Byte (Thumb, 100 bytes, Stack size 16 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> IIC_NAck
  - >> IIC_Ack
  - >> delay_us
  [Called By]
  - >> AT24C02_ReadOneByte

  AT24C02_ReadOneByte (Thumb, 88 bytes, Stack size 16 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> IIC_Read_Byte
  - >> IIC_Send_Byte
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  [Called By]
  - >> AT24C02_Check
  - >> AT24C02_ReadLenByte
  - >> AT24C02_Read

  AT24C02_WriteOneByte (Thumb, 80 bytes, Stack size 16 bytes, 24c02.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = AT24C02_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> delay_ms
  - >> IIC_Send_Byte
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  [Called By]
  - >> AT24C02_Write
  - >> AT24C02_Check
  - >> AT24C02_Erase_Zero
  - >> AT24C02_WriteLenByte
  - >> Para_Write

  AT24C02_WriteLenByte (Thumb, 42 bytes, Stack size 24 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> AT24C02_WriteOneByte

  AT24C02_ReadLenByte (Thumb, 44 bytes, Stack size 24 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> AT24C02_ReadOneByte

  AT24C02_Erase_Zero (Thumb, 24 bytes, Stack size 8 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> AT24C02_WriteOneByte
  [Called By]
  - >> AT24C02_Check

  AT24C02_Check (Thumb, 52 bytes, Stack size 8 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> AT24C02_Erase_Zero
  - >> AT24C02_ReadOneByte
  - >> AT24C02_WriteOneByte

  AT24C02_Read (Thumb, 34 bytes, Stack size 16 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> AT24C02_ReadOneByte
  [Called By]
  - >> cmd_para_init

  AT24C02_Write (Thumb, 36 bytes, Stack size 16 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> AT24C02_WriteOneByte

  AT24C02_Init (Thumb, 8 bytes, Stack size 8 bytes, 24c02.o(.text), UNUSED)
  [Calls]

  - >> IIC_Init

  open_sim800_pwr (Thumb, 42 bytes, Stack size 8 bytes, sim800c.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = open_sim800_pwr ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> main

  com_usart1 (Thumb, 150 bytes, Stack size 32 bytes, sim800c.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = com_usart1 ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_Init
  - >> GPIO_Init
  - >> NVIC_Init
  [Called By]
  - >> main

  USART1_IRQHandler (Thumb, 80 bytes, Stack size 8 bytes, sim800c.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ClearITPendingBit
  - >> USART_GetITStatus
  - >> USART_ReceiveData
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  sim800_send (Thumb, 66 bytes, Stack size 16 bytes, sim800c.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = sim800_send
  [Calls]
  - >> USART_GetFlagStatus
  - >> USART_SendData
  - >> __aeabi_memclr
  [Called By]
  - >> init_sim800
  - >> net_send

  check_init_state (Thumb, 32 bytes, Stack size 8 bytes, sim800c.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = check_init_state ⇒ __2printf
  [Calls]
  - >> SystemReset
  - >> __2printf
  [Called By]
  - >> init_sim800

  init_sim800 (Thumb, 640 bytes, Stack size 8 bytes, sim800c.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = init_sim800 ⇒ check_init_state ⇒ __2printf
  [Calls]
  - >> strncmp
  - >> check_init_state
  - >> sim800_send
  - >> __2printf
  [Called By]
  - >> sim800_run

  sim800_recevie (Thumb, 472 bytes, Stack size 8 bytes, sim800c.o(.text), UNUSED)
  [Calls]

  - >> net_buffer_input

  sim800_run (Thumb, 146 bytes, Stack size 16 bytes, sim800c.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = sim800_run ⇒ init_sim800 ⇒ check_init_state ⇒ __2printf
  [Calls]
  - >> __aeabi_memclr
  - >> init_sim800
  - >> net_buffer_input
  - >> __2printf
  [Called By]
  - >> main

  GPIO_Configuration (Thumb, 72 bytes, Stack size 8 bytes, device.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init

  Reset_W5500 (Thumb, 36 bytes, Stack size 8 bytes, device.o(.text), UNUSED)
  [Calls]

  - >> Delay_ms
  - >> GPIO_ResetBits
  - >> GPIO_SetBits

  reboot (Thumb, 12 bytes, Stack size 16 bytes, device.o(.text), UNUSED)

  set_network (Thumb, 370 bytes, Stack size 32 bytes, device.o(.text), UNUSED)
  [Calls]

  - >> Delay_ms
  - >> sysinit
  - >> setSUBR
  - >> setSIPR
  - >> setSHAR
  - >> setRTR
  - >> setRCR
  - >> setGAR
  - >> getSUBR
  - >> getSIPR
  - >> getSHAR
  - >> getPHYStatus
  - >> getGAR
  - >> __2printf

  set_default (Thumb, 168 bytes, Stack size 40 bytes, device.o(.text), UNUSED)
  [Calls]

  - >> at24c16_read
  - >> __2printf

  set_default_reset (Thumb, 122 bytes, Stack size 32 bytes, device.o(.text), UNUSED)
  [Called By]

  - >> key_process

  IINCHIP_CSon (Thumb, 10 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> WIZ_CS
  [Called By]
  - >> wiz_read_buf
  - >> wiz_write_buf
  - >> IINCHIP_READ
  - >> IINCHIP_WRITE

  IINCHIP_SpiSendData (Thumb, 12 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> SPI2_SendByte
  [Called By]
  - >> wiz_read_buf
  - >> wiz_write_buf
  - >> IINCHIP_READ
  - >> IINCHIP_WRITE

  IINCHIP_CSoff (Thumb, 10 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> WIZ_CS
  [Called By]
  - >> wiz_read_buf
  - >> wiz_write_buf
  - >> IINCHIP_READ
  - >> IINCHIP_WRITE

  IINCHIP_WRITE (Thumb, 50 bytes, Stack size 16 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_CSoff
  - >> IINCHIP_SpiSendData
  - >> IINCHIP_CSon
  [Called By]
  - >> setSn_IR
  - >> recv_data_processing
  - >> send_data_processing
  - >> setSn_TTL
  - >> setSn_MSS
  - >> clearIR
  - >> setMR
  - >> setkeepalive
  - >> sysinit
  - >> setRTR
  - >> setRCR

  setkeepalive (Thumb, 20 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_WRITE

  getISR (Thumb, 8 bytes, Stack size 0 bytes, w5500.o(.text), UNUSED)

  putISR (Thumb, 6 bytes, Stack size 0 bytes, w5500.o(.text), UNUSED)

  getIINCHIP_RxMAX (Thumb, 10 bytes, Stack size 0 bytes, w5500.o(.text), UNUSED)

  getIINCHIP_TxMAX (Thumb, 10 bytes, Stack size 0 bytes, w5500.o(.text), UNUSED)

  IINCHIP_READ (Thumb, 50 bytes, Stack size 16 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_CSoff
  - >> IINCHIP_SpiSendData
  - >> IINCHIP_CSon
  [Called By]
  - >> recv_data_processing
  - >> send_data_processing
  - >> getSn_RX_RSR
  - >> getSn_TX_FSR
  - >> getSn_SR
  - >> getSn_IR
  - >> getIR
  - >> getPHYStatus

  wiz_write_buf (Thumb, 72 bytes, Stack size 24 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_CSoff
  - >> IINCHIP_SpiSendData
  - >> IINCHIP_CSon
  [Called By]
  - >> send_data_processing
  - >> setSUBR
  - >> setSIPR
  - >> setSHAR
  - >> setGAR

  wiz_read_buf (Thumb, 70 bytes, Stack size 24 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_CSoff
  - >> IINCHIP_SpiSendData
  - >> IINCHIP_CSon
  [Called By]
  - >> recv_data_processing
  - >> getGWIP
  - >> getSUBR
  - >> getSIPR
  - >> getSHAR
  - >> getGAR

  setMR (Thumb, 14 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_WRITE
  [Called By]
  - >> iinchip_init

  iinchip_init (Thumb, 10 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> setMR

  sysinit (Thumb, 302 bytes, Stack size 24 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_WRITE
  [Called By]
  - >> set_network

  setGAR (Thumb, 16 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> wiz_write_buf
  [Called By]
  - >> set_network

  getGWIP (Thumb, 16 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> wiz_read_buf

  setSUBR (Thumb, 18 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> wiz_write_buf
  [Called By]
  - >> set_network

  setSHAR (Thumb, 18 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> wiz_write_buf
  [Called By]
  - >> set_network

  setSIPR (Thumb, 18 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> wiz_write_buf
  [Called By]
  - >> set_network

  getGAR (Thumb, 16 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> wiz_read_buf
  [Called By]
  - >> set_network

  getSUBR (Thumb, 18 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> wiz_read_buf
  [Called By]
  - >> set_network

  getSHAR (Thumb, 18 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> wiz_read_buf
  [Called By]
  - >> set_network

  getSIPR (Thumb, 18 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> wiz_read_buf
  [Called By]
  - >> set_network

  getIR (Thumb, 12 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_READ
  [Called By]
  - >> clearIR

  setRTR (Thumb, 26 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_WRITE
  [Called By]
  - >> set_network

  setRCR (Thumb, 16 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_WRITE
  [Called By]
  - >> set_network

  clearIR (Thumb, 26 bytes, Stack size 16 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> getIR
  - >> IINCHIP_WRITE

  setSn_MSS (Thumb, 36 bytes, Stack size 16 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_WRITE

  setSn_TTL (Thumb, 22 bytes, Stack size 16 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_WRITE

  getSn_IR (Thumb, 18 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_READ

  getSn_SR (Thumb, 18 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_READ

  getSn_TX_FSR (Thumb, 84 bytes, Stack size 16 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_READ

  getSn_RX_RSR (Thumb, 100 bytes, Stack size 16 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_READ

  send_data_processing (Thumb, 108 bytes, Stack size 24 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> wiz_write_buf
  - >> IINCHIP_READ
  - >> IINCHIP_WRITE

  recv_data_processing (Thumb, 108 bytes, Stack size 24 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> wiz_read_buf
  - >> IINCHIP_READ
  - >> IINCHIP_WRITE

  setSn_IR (Thumb, 22 bytes, Stack size 16 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_WRITE

  getPHYStatus (Thumb, 12 bytes, Stack size 8 bytes, w5500.o(.text), UNUSED)
  [Calls]

  - >> IINCHIP_READ
  [Called By]
  - >> set_network

  WIZ_SPI_Init (Thumb, 154 bytes, Stack size 32 bytes, spi2.o(.text), UNUSED)
  [Calls]

  - >> SPI_Cmd
  - >> SPI_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init

  WIZ_CS (Thumb, 30 bytes, Stack size 8 bytes, spi2.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> IINCHIP_CSoff
  - >> IINCHIP_CSon

  SPI2_SendByte (Thumb, 50 bytes, Stack size 8 bytes, spi2.o(.text), UNUSED)
  [Calls]

  - >> SPI_I2S_GetFlagStatus
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_SendData
  [Called By]
  - >> IINCHIP_SpiSendData

  Delay_us (Thumb, 42 bytes, Stack size 12 bytes, 24c16.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Delay_us
  [Called By]
  - >> timer2_irq
  - >> at24c16_start
  - >> write_1byte
  - >> clock
  - >> read_1byte
  - >> at24c16_stop

  at24c16_stop (Thumb, 40 bytes, Stack size 8 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> Delay_us
  [Called By]
  - >> at24c16_write
  - >> at24c16_read

  read_1byte (Thumb, 110 bytes, Stack size 16 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_ReadInputDataBit
  - >> Delay_us
  [Called By]
  - >> at24c16_read

  clock (Thumb, 62 bytes, Stack size 8 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_ReadInputDataBit
  - >> Delay_us
  [Called By]
  - >> at24c16_write
  - >> at24c16_read

  write_1byte (Thumb, 122 bytes, Stack size 16 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> Delay_us
  [Called By]
  - >> at24c16_write
  - >> at24c16_read

  at24c16_start (Thumb, 50 bytes, Stack size 8 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> Delay_us
  [Called By]
  - >> at24c16_write
  - >> at24c16_read

  at24c16_read (Thumb, 70 bytes, Stack size 16 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> at24c16_start
  - >> write_1byte
  - >> clock
  - >> read_1byte
  - >> at24c16_stop
  [Called By]
  - >> load_ip_pri
  - >> eeprom_read
  - >> set_default

  eeprom_read (Thumb, 36 bytes, Stack size 24 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> at24c16_read
  [Called By]
  - >> load_ip_pri

  at24c16_write (Thumb, 80 bytes, Stack size 16 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> Delay_ms
  - >> at24c16_start
  - >> write_1byte
  - >> clock
  - >> at24c16_stop
  [Called By]
  - >> write_eeprom_flag
  - >> erase_eeprom
  - >> eep_block_write
  - >> clear_eeprom_flag
  - >> eeprom_write

  eeprom_write (Thumb, 36 bytes, Stack size 24 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> at24c16_write
  [Called By]
  - >> write_ip_pri

  write_ip_pri (Thumb, 14 bytes, Stack size 8 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> eeprom_write
  [Called By]
  - >> key_process

  load_ip_pri (Thumb, 56 bytes, Stack size 8 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> eeprom_read
  - >> at24c16_read
  - >> __2printf
  [Called By]
  - >> at24c16_init

  write_eeprom_flag (Thumb, 20 bytes, Stack size 8 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> at24c16_write
  [Called By]
  - >> key_process

  clear_eeprom_flag (Thumb, 20 bytes, Stack size 8 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> at24c16_write

  at24c16_init (Thumb, 72 bytes, Stack size 8 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> load_ip_pri

  eep_block_write (Thumb, 40 bytes, Stack size 24 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> at24c16_write

  erase_eeprom (Thumb, 30 bytes, Stack size 16 bytes, 24c16.o(.text), UNUSED)
  [Calls]

  - >> at24c16_write

  fan_on (Thumb, 18 bytes, Stack size 8 bytes, hcho.o(.text), UNUSED)
  [Calls]

  - >> GPIO_SetBits

  fan_off (Thumb, 18 bytes, Stack size 8 bytes, hcho.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ResetBits

  fan_init (Thumb, 38 bytes, Stack size 8 bytes, hcho.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init

  hcho_is_ok (Thumb, 38 bytes, Stack size 8 bytes, hcho.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ReadInputDataBit
  - >> GPIO_Init

  hcho_adc_Init (Thumb, 168 bytes, Stack size 32 bytes, hcho.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = hcho_adc_Init ⇒ GPIO_Init
  [Calls]
  - >> ADC_TempSensorVrefintCmd
  - >> ADC_GetCalibrationStatus
  - >> ADC_StartCalibration
  - >> ADC_GetResetCalibrationStatus
  - >> ADC_ResetCalibration
  - >> ADC_Cmd
  - >> ADC_Init
  - >> ADC_DeInit
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  hcho_adc_sample (Thumb, 66 bytes, Stack size 8 bytes, hcho.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = hcho_adc_sample ⇒ __2printf
  [Calls]
  - >> ADC_ClearFlag
  - >> ADC_GetFlagStatus
  - >> ADC_GetConversionValue
  - >> ADC_RegularChannelConfig
  - >> ADC_SoftwareStartConvCmd
  - >> __2printf
  [Called By]
  - >> timer2_irq

  hm_adc_sample (Thumb, 66 bytes, Stack size 8 bytes, hcho.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = hm_adc_sample ⇒ __2printf
  [Calls]
  - >> ADC_ClearFlag
  - >> ADC_GetFlagStatus
  - >> ADC_GetConversionValue
  - >> ADC_RegularChannelConfig
  - >> ADC_SoftwareStartConvCmd
  - >> __2printf
  [Called By]
  - >> timer2_irq

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> ZLN_Read
  - >> server_send
  - >> DES
  - >> P
  - >> RShift
  - >> LShift
  - >> EP
  - >> IP
  - >> server_get_id
  - >> app_process_cmd
  - >> Operate_SET_ALL
  - >> Operate_SET_PORT
  - >> Operate_SET_ALARM
  - >> Operate_SET_SW
  - >> Operate_GET_NONC
  - >> Operate_SET_NONC
  - >> Operate_GET_INPUT
  - >> Operate_STATE
  - >> Operate_READ_RELAY
  - >> Operate_SET_RELAY

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text))
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> sim800_run
  - >> sim800_send
  - >> app_process_cmd
  - >> Operate_SET_ALL
  - >> Operate_SET_PORT
  - >> Operate_SET_ALARM
  - >> Operate_SET_SW
  - >> Operate_GET_NONC
  - >> Operate_SET_NONC
  - >> Operate_GET_INPUT
  - >> Operate_STATE
  - >> Operate_READ_RELAY
  - >> Operate_SET_RELAY

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> Send_Alarm_Message
  - >> timer_all_init
  - >> server_host_id
  - >> server_client_clr
  - >> net_val_init
  - >> sync_data
  - >> server_send
  - >> com_cmd_handle
  - >> net_cmd_handle
  - >> clr_buf
  - >> com_val_init
  - >> Net_SendReply
  - >> app_process_cmd
  - >> Operate_HOST
  - >> Operate_SCAN_DEVICE
  - >> Operate_SET_ALL
  - >> Operate_SET_PORT
  - >> Operate_SET_ALARM
  - >> Operate_SET_SW
  - >> Operate_GET_NONC
  - >> Operate_SET_NONC
  - >> Operate_GET_INPUT
  - >> Operate_STATE
  - >> Operate_READ_RELAY
  - >> Operate_SET_RELAY

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strcat (Thumb, 24 bytes, Stack size 0 bytes, strcat.o(.text))
  [Called By]

  - >> Net_SendReply

  strchr (Thumb, 20 bytes, Stack size 0 bytes, strchr.o(.text))
  [Called By]

  - >> SplitData
  - >> app_process_cmd
  - >> Operate_SET_ALL
  - >> Operate_SET_PORT
  - >> Operate_ALARM
  - >> Operate_READ_RELAY

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> sync_data
  - >> Net_SendReply
  - >> Operate_HOST

  strcmp (Thumb, 28 bytes, Stack size 8 bytes, strcmp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strcmp
  [Called By]
  - >> app_process_cmd
  - >> Operate_ALARM

  memcmp (Thumb, 26 bytes, Stack size 12 bytes, memcmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = memcmp
  [Called By]
  - >> server_handle
  - >> server_add_client
  - >> server_check_lic

  strncmp (Thumb, 30 bytes, Stack size 12 bytes, strncmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strncmp
  [Called By]
  - >> init_sim800

  atoi (Thumb, 26 bytes, Stack size 16 bytes, atoi.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> strtol
  - >> __aeabi_errno_addr
  [Called By]
  - >> SplitData
  - >> Operate_SET_ALL
  - >> Operate_SET_PORT
  - >> Operate_GET_NONC
  - >> Operate_ALARM
  - >> Operate_GET_INPUT
  - >> Operate_STATE
  - >> Operate_READ_RELAY

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  strtol (Thumb, 112 bytes, Stack size 32 bytes, strtol.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = strtol ⇒ _strtoul
  [Calls]
  - >> _strtoul
  - >> __rt_ctype_table
  - >> __aeabi_errno_addr
  [Called By]
  - >> atoi

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __rt_ctype_table (Thumb, 4 bytes, Stack size 0 bytes, ctype_o.o(.text))
  [Called By]

  - >> strtol

  _strtoul (Thumb, 158 bytes, Stack size 40 bytes, _strtoul.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _strtoul
  [Calls]
  - >> _chval
  - >> __aeabi_errno_addr
  [Called By]
  - >> strtol

  _chval (Thumb, 28 bytes, Stack size 0 bytes, _chval.o(.text))
  [Called By]

  - >> _strtoul

  __0printf$8 (Thumb, 22 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$8 (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> key_process
  - >> sim800_run
  - >> main
  - >> load_ip_pri
  - >> set_default
  - >> set_network
  - >> init_sim800
  - >> check_init_state
  - >> hm_adc_sample
  - >> hcho_adc_sample
  - >> sync_data
  - >> server_heartbeat
  - >> server_login
  - >> server_handle
  - >> Net_SendReply
  - >> app_process_cmd
  - >> Operate_READ_RELAY

  __0sprintf$8 (Thumb, 34 bytes, Stack size 24 bytes, printf8.o(i.__0sprintf$8), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf$8 (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0sprintf$8), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0sprintf$8))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> Send_Alarm_Message
  - >> sync_data
  - >> server_read_mcu_id
  - >> Operate_HOST
  - >> Operate_SCAN_DEVICE
  - >> Operate_SET_ALL
  - >> Operate_SET_PORT
  - >> Operate_SET_ALARM
  - >> Operate_SET_SW
  - >> Operate_GET_NONC
  - >> Operate_SET_NONC
  - >> Operate_GET_INPUT
  - >> Operate_STATE
  - >> Operate_READ_RELAY
  - >> Operate_SET_RELAY

  __aeabi_errno_addr (Thumb, 4 bytes, Stack size 0 bytes, errno.o(i.__aeabi_errno_addr))
  [Called By]

  - >> _strtoul
  - >> strtol
  - >> atoi

  __rt_errno_addr (Thumb, 0 bytes, Stack size 0 bytes, errno.o(i.__aeabi_errno_addr), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  TI4_Config (Thumb, 130 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI3_Config (Thumb, 122 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI2_Config (Thumb, 130 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TI1_Config (Thumb, 108 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  set_alarm (Thumb, 238 bytes, Stack size 16 bytes, app_processevents.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> SET_RELAY

  Test_Relay (Thumb, 84 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Test_Relay
  [Calls]
  - >> delay_ms
  [Called By]
  - >> Operate_HOST

  read_input (Thumb, 46 bytes, Stack size 16 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = read_input
  [Called By]
  - >> Operate_GET_INPUT

  Switch_State_Scan (Thumb, 230 bytes, Stack size 8 bytes, app_processevents.o(.text), UNUSED)
  [Calls]

  - >> timer_signal_set
  - >> timer_get_state
  [Called By]
  - >> alarm_process

  Send_Alarm_Message (Thumb, 46 bytes, Stack size 40 bytes, app_processevents.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memclr4
  - >> Net_SendReply
  - >> __2sprintf
  [Called By]
  - >> Alarm_Resend
  - >> alarm_process

  Parameter_Check (Thumb, 34 bytes, Stack size 0 bytes, app_processevents.o(.text))
  [Called By]

  - >> Operate_SET_ALARM
  - >> Operate_SET_SW
  - >> Operate_SET_NONC
  - >> Operate_ALARM
  - >> Operate_READ_RELAY
  - >> Operate_SET_RELAY

  Get_Set (Thumb, 134 bytes, Stack size 8 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Get_Set
  [Called By]
  - >> Operate_GET_NONC
  - >> Operate_STATE
  - >> SET_RELAY

  SplitData (Thumb, 106 bytes, Stack size 40 bytes, app_processevents.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = SplitData ⇒ atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> strchr
  - >> atoi
  [Called By]
  - >> Operate_SET_ALARM
  - >> Operate_SET_SW
  - >> Operate_SET_NONC
  - >> Operate_SET_RELAY

  ExpandBit (Thumb, 46 bytes, Stack size 12 bytes, des.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = ExpandBit
  [Called By]
  - >> DES
  - >> InitKey

  ShrinkBit (Thumb, 58 bytes, Stack size 12 bytes, des.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = ShrinkBit
  [Called By]
  - >> DES

  Xor (Thumb, 24 bytes, Stack size 12 bytes, des.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Xor
  [Called By]
  - >> DES

  IP (Thumb, 36 bytes, Stack size 16 bytes, des.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IP
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> DES

  EP (Thumb, 36 bytes, Stack size 16 bytes, des.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = EP
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> DES

  InitKey (Thumb, 36 bytes, Stack size 16 bytes, des.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = InitKey ⇒ ExpandBit
  [Calls]
  - >> ExpandBit
  [Called By]
  - >> DES

  LShift (Thumb, 54 bytes, Stack size 16 bytes, des.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = LShift
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> SubKey

  RShift (Thumb, 54 bytes, Stack size 16 bytes, des.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = RShift
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> SubKey

  SubKey (Thumb, 90 bytes, Stack size 24 bytes, des.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SubKey ⇒ RShift
  [Calls]
  - >> RShift
  - >> LShift
  [Called By]
  - >> DES

  EXP (Thumb, 22 bytes, Stack size 0 bytes, des.o(.text))
  [Called By]

  - >> DES

  S (Thumb, 122 bytes, Stack size 20 bytes, des.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = S
  [Called By]
  - >> DES

  P (Thumb, 36 bytes, Stack size 16 bytes, des.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = P
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> DES

  _printf_core (Thumb, 996 bytes, Stack size 104 bytes, printf8.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  [Called By]
  - >> __0sprintf$8
  - >> __0printf$8

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printf8.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printf8.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printf8.o(i._sputc))
  [Called By]

  - >> __0sprintf$8
  [Address Reference Count : 1]
  - printf8.o(i.__0sprintf$8)

  ### Undefined Global Symbols