*************************** START ****************************

START TIME: 202210311505

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa404698
mac h: 0x65b48a
crc_cal: 101
crc_read: 101
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 901.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2454.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7374.1 kbit/s)...

Hash of data verified.
Wrote 677952 bytes (412855 compressed) at 0x00010000 in 6.9 seconds (effective 789.0 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 10 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202210311537

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa404698
mac h: 0x65b48a
crc_cal: 101
crc_read: 101
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 905.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2478.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7866.7 kbit/s)...

Hash of data verified.
Wrote 677952 bytes (412855 compressed) at 0x00010000 in 6.9 seconds (effective 788.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 9 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202211020946

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa404698
mac h: 0x65b48a
crc_cal: 101
crc_read: 101
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 902.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2454.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7393.8 kbit/s)...

Hash of data verified.
Wrote 677952 bytes (412858 compressed) at 0x00010000 in 7.0 seconds (effective 777.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 9 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202211020946

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa404698
mac h: 0x65b48a
crc_cal: 101
crc_read: 101
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 901.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2655.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 8048.4 kbit/s)...

Hash of data verified.
Wrote 677952 bytes (412855 compressed) at 0x00010000 in 7.0 seconds (effective 778.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 9 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202211020947

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa404698
mac h: 0x65b48a
crc_cal: 101
crc_read: 101
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 896.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2472.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7310.2 kbit/s)...

Hash of data verified.
Wrote 677952 bytes (412858 compressed) at 0x00010000 in 7.0 seconds (effective 779.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 10 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202211021121

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa404698
mac h: 0x65b48a
crc_cal: 101
crc_read: 101
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 901.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2522.9 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7492.7 kbit/s)...

Hash of data verified.
Wrote 677968 bytes (412989 compressed) at 0x00010000 in 6.7 seconds (effective 807.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 9 s

Download result: PASS

*************************** END ****************************



