*************************** START ****************************

START TIME: 202211070855

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55135a50
mac h: 0x4c94b5
crc_cal: 76
crc_read: 76
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.1 seconds (effective 913.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2733.3 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 8201.4 kbit/s)...

Hash of data verified.
Wrote 677968 bytes (412989 compressed) at 0x00010000 in 6.5 seconds (effective 829.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 9 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202211101317

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55135a50
mac h: 0x4c94b5
crc_cal: 76
crc_read: 76
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 913.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2457.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7583.3 kbit/s)...

Hash of data verified.
Wrote 723072 bytes (448446 compressed) at 0x00010000 in 6.9 seconds (effective 843.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 9 s

Download result: PASS

*************************** END ****************************



