*************************** START ****************************

START TIME: 202212121036

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a68bb4
mac h: 0x408c4b
crc_cal: 64
crc_read: 64
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 907.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2761.4 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7953.9 kbit/s)...

Hash of data verified.
Wrote 738688 bytes (420689 compressed) at 0x00010000 in 8.0 seconds (effective 737.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202212121037

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a68bb4
mac h: 0x408c4b
crc_cal: 64
crc_read: 64
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.1 seconds (effective 914.0 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2802.7 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 8432.9 kbit/s)...

Hash of data verified.
Wrote 678240 bytes (413437 compressed) at 0x00010000 in 7.5 seconds (effective 723.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 10 s

Download result: PASS

*************************** END ****************************



