*************************** START ****************************

START TIME: 202301111513

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a6d5f4
mac h: 0xad8c4b
crc_cal: 173
crc_read: 173
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 838.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 1461.1 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 3991.0 kbit/s)...

Hash of data verified.
Wrote 273152 bytes (119457 compressed) at 0x00010000 in 2.8 seconds (effective 784.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 5 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202302081024

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a6d5f4
mac h: 0xad8c4b
crc_cal: 173
crc_read: 173
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 904.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2554.4 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7658.9 kbit/s)...

Hash of data verified.
Wrote 833856 bytes (526522 compressed) at 0x00010000 in 9.1 seconds (effective 735.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202302081026

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a6d5f4
mac h: 0xad8c4b
crc_cal: 173
crc_read: 173
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 833856 bytes (526522 compressed) at 0x00000000 in 9.1 seconds (effective 735.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202302081028

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a6d5f4
mac h: 0xad8c4b
crc_cal: 173
crc_read: 173
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 907.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2578.3 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7686.3 kbit/s)...

Hash of data verified.
Wrote 833856 bytes (526522 compressed) at 0x00010000 in 9.0 seconds (effective 737.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202302081031

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a6d5f4
mac h: 0xad8c4b
crc_cal: 173
crc_read: 173
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 907.1 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2545.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7957.8 kbit/s)...

Hash of data verified.
Wrote 833856 bytes (526522 compressed) at 0x00010000 in 9.0 seconds (effective 738.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202302081123

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a6d5f4
mac h: 0xad8c4b
crc_cal: 173
crc_read: 173
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 913.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2573.8 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7549.9 kbit/s)...

Hash of data verified.
Wrote 844080 bytes (483716 compressed) at 0x00010000 in 9.0 seconds (effective 752.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202302081124

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a6d5f4
mac h: 0xad8c4b
crc_cal: 173
crc_read: 173
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 907.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2553.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7654.6 kbit/s)...

Hash of data verified.
Wrote 844080 bytes (483716 compressed) at 0x00010000 in 9.0 seconds (effective 753.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



