*************************** START ****************************

START TIME: 202212291003

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a650d8
mac h: 0xfd8c4b
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 907.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2543.7 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7284.6 kbit/s)...

Hash of data verified.
Wrote 971872 bytes (639598 compressed) at 0x00010000 in 10.6 seconds (effective 736.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202212291003

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a650d8
mac h: 0xfd8c4b
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 971872 bytes (639598 compressed) at 0x00010000 in 10.5 seconds (effective 741.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202212291003

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a650d8
mac h: 0xfd8c4b
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 908.0 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2431.5 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7875.0 kbit/s)...

Hash of data verified.
Wrote 971872 bytes (639598 compressed) at 0x00010000 in 10.5 seconds (effective 743.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202212291031

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a650d8
mac h: 0xfd8c4b
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 905.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2619.4 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7840.7 kbit/s)...

Hash of data verified.
Wrote 971872 bytes (639598 compressed) at 0x00010000 in 10.5 seconds (effective 743.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202212291034

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a650d8
mac h: 0xfd8c4b
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 912.5 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2405.1 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7670.2 kbit/s)...

Hash of data verified.
Wrote 971872 bytes (639598 compressed) at 0x00010000 in 10.5 seconds (effective 743.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202212291037

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a650d8
mac h: 0xfd8c4b
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 907.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2585.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7773.5 kbit/s)...

Hash of data verified.
Wrote 971872 bytes (639598 compressed) at 0x00010000 in 10.4 seconds (effective 744.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202212291039

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a650d8
mac h: 0xfd8c4b
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 907.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 2797.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 7576.4 kbit/s)...

Hash of data verified.
Wrote 971872 bytes (639598 compressed) at 0x00010000 in 10.5 seconds (effective 743.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



