*************************** START ****************************

START TIME: 202301111522

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x14a6cca4
mac h: 0x288c4b
crc_cal: 40
crc_read: 40
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17136 bytes (11584 compressed) at 0x00001000 in 0.2 seconds (effective 831.7 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 1406.4 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 4136.4 kbit/s)...

Hash of data verified.
Wrote 273152 bytes (119457 compressed) at 0x00010000 in 2.8 seconds (effective 772.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 5 s

Download result: PASS

*************************** END ****************************



